{"text_format":"1","workbook":"xlsx","n_sheets":8,"sheets":["Head","Input","Output","Key figures","Lists, etc.","Intro","BaseIDs","Parameters and examples"],"not_rendered":{"charts":0,"images":4,"macros":1,"external_links":0,"defined_names":75,"comments":3,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Head","index":0,"n_rows":18,"n_cols":3,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
[null,20190317]
[]
[]
["General project information (Head section)"]
[]
["Path, energyPRO:","c:\\Program Files\\EMD\\energyPRO 4\\energyPRO4.exe"]
["Project file, xml file and reports in same path as spreadsheet:","yes"]
["Name, project file:"]
["Path, project file:","C:\\INTERFACE\\"]
["Path, xml file:","C:\\INTERFACE\\"]
["Path, report files:","C:\\INTERFACE\\"]
["Name, xml file:","input"]
["Calculate:","True"]
["Spool:","True"]
["Save:","False",false]
["SaveAs:"]
["Date",{"$f":"NOW()","v":"2019-03-17T12:42:26.980"}]
["Version","1"]

{"sheet":"Input","index":1,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["Modifying input (input section)"]
[]
["Start run number",1]
["End run number",1]
["Input ID"]
["Data element"]
["Sub data element"]
["COMPARE, name of alternative"]
["Parameter name (corresponding to name in the energyPRO model)"]
["Time series file type"]
["File field delimiter"]
["Data element index"]
[2,{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0},{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0},{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0},{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0},{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0},{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0},{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0},{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0}]
["Present calculation:↗"]
["Run","Parameter 1","Parameter 2","Parameter 3","Parameter 4","Parameter 5","Parameter 6","Parameter 7","Parameter 8"]
[1]
[2]
[3]
[4]
[5]
[6]

{"sheet":"Output","index":2,"n_rows":15,"n_cols":2,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["Requested reports (output section)"]
[]
["Output Report Type","Text report"]
["Report ID","EnergyConversionAnnual"]
["COMPARE, name of alternative"]
["Report name"]
["Report extension","txt"]
["Report delimiter"]
["Report decimal separator"]
["Report Resolution"]
["Report start date"]
["Report end date"]

{"sheet":"Key figures","index":3,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
["Report #"]
["row"]
["item"]
[]
[null,"2017-11-10T11:10:17"]
["Run","Column1","Column2","Column3","Column4","Column5","Column6","Column7","Column8","Column9"]
[1]
[2]
[3]
[4]
[5]
[6]

{"sheet":"Lists, etc.","index":4,"n_rows":181,"n_cols":11,"rows_kept":181,"cut":false,"hidden":true,"merged":[]}
[null,"Input types","Dataelements",null,"<?xml version=\"1.0\"?>"]
[null,"ProjectIdentificationData","ProjectIdentificationData","BaseID"]
[null,"ExternalConditionData","ExternalConditionData","BaseID"]
[null,"TimeSeriesData","TimeSeriesData","BaseID"]
[null,"TimeSeriesFunctionData","TimeSeriesFunctionData","BaseID"]
[null,"TransmissionData","TransmissionData","BaseID"]
[null,"FuelData","FuelData","BaseID"]
[null,"DemandData","DemandData","BaseID"]
[null,"EnergyConversionUnitData","EnergyConversionUnitData","BaseID"]
[null,"StorageData","StorageData","BaseID"]
[null,"EnvironmentData","EnvironmentData","BaseID"]
[null,"EconomyData","EconomyData","BaseID"]
[null,"FinancingData","FinancingData","BaseID"]
[null,"TaxationData","TaxationData","BaseID"]
[null,"ProjectFile","ProjectFile","Head"]
[]
[null,null,null,"DataName","AltName"]
[null,"ProjectIdentificationData"]
[null,"ID.Strings",null,"DataElementName","DataElementValue"]
[null,"CalcPeriodlengthMinutes",null,"DataElementName","DataElementValue"]
[null,"OptimizationPeriodLength",null,"DataElementName","DataElementValue"]
[]
[]
[null,"ExternalConditionData"]
[null,"CalcStart",null,"DataElementName","DataElementTimeValue"]
[null,"CalcEnd",null,"DataElementName","DataElementTimeValue"]
[]
[]
[null,"TimeSeriesData"]
[null,"Weatherdata.TimeSeries",null,"DataElementName","TimeSeriesFileName","TimeSeriesFileTypes"]
[null,"IsInDaylightSaving",null,"DataElementName","DataElementValue","txt",null,null,"TimeSeriesFileType"]
[null,"Latitude",null,"DataElementName","DataElementValue","csv",null,null,"ReportDelimiter"]
[null,"Longitude",null,"DataElementName","DataElementValue","epw"]
[null,"DevelopingFlag",null,"DataElementName","DataElementValue","xml"]
[]
[]
[null,"TimeSeriesFunctionData"]
[null,"FuncFormular",null,"DataElementName","DataElementValue"]
[null,"Latitude",null,"DataElementName","DataElementValue"]
[null,"Longitude",null,"DataElementName","DataElementValue"]
[null,"WeatherUnit",null,"DataElementName","DataElementValue"]
[]
[]
[null,"FuelData"]
[null,"ThermalValue",null,"DataElementName","DataElementValue"]
[null,"UnitName",null,"DataElementName","DataElementValue"]
[null,"FuelStorage",null,"DataElementName","DataElementValue"]
[]
[]
[null,"TransmissionData"]
[null,"SiteAtoB",null,"DataElementName","DataElementValue"]
[null,"SiteBtoA",null,"DataElementName","DataElementValue"]
[null,"Capacity",null,"DataElementName","DataElementValue"]
[null,"Loss",null,"DataElementName","DataElementValue"]
[null,"NonAvailableTimes.StartTime",null,"DataElementName","DataElementTimeValue"]
[null,"NonAvailableTimes.EndTime",null,"DataElementName","DataElementTimeValue"]
[null,"NonAvailableTimes.Occurrence",null,"DataElementName","DataElementValue"]
[null,"OperationalFrom",null,"DataElementName","DataElementTimeValue"]
[null,"OperationalTo",null,"DataElementName","DataElementTimeValue"]
[]
[]
[null,"DemandData"]
[null,"Demand",null,"DataElementName","DataElementValue"]
[null,"OutDoorTempSymbol",null,"DataElementName","DataElementValue"]
[null,"ReferenceTemperature",null,"DataElementName","DataElementValue"]
[null,"WeatherDepFraction",null,"DataElementName","DataElementValue"]
[null,"WeatherDepSeasonFrom",null,"DataElementName","DataElementTimeValue"]
[null,"WeatherDepSeasonTo",null,"DataElementName","DataElementTimeValue"]
[null,"DemandFrom",null,"DataElementName","DataElementTimeValue"]
[null,"IncludedFrom",null,"DataElementName","DataElementTimeValue"]
[null,"IncludedTo",null,"DataElementName","DataElementTimeValue"]
[null,"SiteID",null,"DataElementName","DataElementValue"]
[null,"Weatherdata.TimeSeries",null,"DataElementName","TimeSeriesFileName"]
[]
[]
[null,"EnergyConversionUnitData","Sub dataelements",null,null,"PowerCurveElements",null,null,null,null,"OccurrenceElements"]
[null,"PowerCurve","PowerCurveElements","DataElementName","DataElementValue","Fuel",null,null,"DataElementValue",null,"once"]
[null,"SolarUnit","SolarUnitElements","DataElementName","DataElementValue","HeatProd",null,null,"DataElementValue",null,"yearly"]
[null,"WindFarm","WindFarmElements","DataElementName","DataElementValue","ElProd",null,null,"DataElementValue",null,"monthly"]
[null,"HeatPump","HeatPumpElements","DataElementName","DataElementTimeValue","CoolProd",null,null,"DataElementValue",null,"weekly"]
[null,"NonAvailableTimes.StartTime",null,"DataElementName","DataElementTimeValue","ProcHeatProd",null,null,"DataElementValue",null,"daily"]
[null,"NonAvailableTimes.EndTime",null,"DataElementName","DataElementValue","HeatCon",null,null,"DataElementValue"]
[null,"NonAvailableTimes.Occurrence",null,"DataElementName","DataElementTimeValue","ElCon",null,null,"DataElementValue"]
[null,"OperationalFrom",null,"DataElementName","DataElementTimeValue","ProcHeatCon",null,null,"DataElementValue"]
[null,"OperationalTo",null,"DataElementName","DataElementValue"]
[null,"StartUpPeriod",null,"DataElementName","DataElementValue"]
[null,"ShutDownPeriod",null,"DataElementName","DataElementValue","SolarUnitElements"]
[null,"MinimumOperatingTime",null,"DataElementName","DataElementValue","TotalArea",null,null,"DataElementValue"]
[null,null,null,null,null,"Inclination",null,null,"DataElementValue"]
[null,null,null,null,null,"Orientation",null,null,"DataElementValue"]
[null,"StorageData",null,null,null,"N0",null,null,"DataElementValue"]
[null,"StorageVolume",null,"DataElementName","DataElementValue","K0",null,null,"DataElementValue"]
[null,"TempTop",null,"DataElementName","DataElementValue","K1",null,null,"DataElementValue"]
[null,"TempBottom",null,"DataElementName","DataElementValue","IncidenceAngleMod50",null,null,"DataElementValue"]
[null,"StorageUtilization",null,"DataElementName","DataElementValue","IncidenceAngleModCoef",null,null,"DataElementValue"]
[null,"StorageHeight",null,"DataElementName","DataElementValue","InstalledElecCapacity",null,null,"DataElementValue"]
[null,"InsulationThickness",null,"DataElementName","DataElementValue","PMax",null,null,"DataElementValue"]
[null,"ThermalConductivity",null,"DataElementName","DataElementValue","TempCoeffPower",null,null,"DataElementValue"]
[null,"AmbientTemperature",null,"DataElementName","DataElementValue","NOCT",null,null,"DataElementValue"]
[null,"HeightDiff",null,"DataElementName","DataElementValue","PowerLosses",null,null,"DataElementValue"]
[null,"WaterReservoirMax",null,"DataElementName","DataElementValue","ForwardTemperature",null,null,"DataElementValue"]
[null,"PumpPowerCapacity",null,"DataElementName","DataElementValue","ReturnTemperature",null,null,"DataElementValue"]
[null,"PumpPowerEfficiency",null,"DataElementName","DataElementValue","TempOnDemandSide",null,null,"DataElementValue"]
[null,"PumpProdCapacity",null,"DataElementName","DataElementValue","NumberOfRows",null,null,"DataElementValue"]
[null,"PumpProdEfficiency",null,"DataElementName","DataElementValue","InclinationGround",null,null,"DataElementValue"]
[null,"MaxBatteryCapacityEX",null,"DataElementName","DataElementValue","DistanceBetweenRows",null,null,"DataElementValue"]
[null,"ECarsCapacityEX",null,"DataElementName","DataElementValue","OrientationGround",null,null,"DataElementValue"]
[null,"InletCapacity",null,"DataElementName","DataElementValue","SolarUnitHeight",null,null,"DataElementValue"]
[null,"OutletCapacity",null,"DataElementName","DataElementValue"]
[null,"InletEfficiency",null,"DataElementName","DataElementValue"]
[null,"OutletEfficiency",null,"DataElementName","DataElementValue","WindFarmElements"]
[null,null,null,null,null,"AnnualProduction",null,null,"DataElementValue"]
[null,null,null,null,null,"WindTSID",null,null,"DataElementValue"]
[null,"EnvironmentData",null,null,null,"MeasureHeight",null,null,"DataElementValue"]
[null,"Amount",null,"DataElementName","DataElementValue","HubHeight",null,null,"DataElementValue"]
[null,null,null,null,null,"ScaleType",null,null,"DataElementValue"]
[null,null,null,null,null,"ScaleValue",null,null,"DataElementValue"]
[null,"EconomyData",null,null,null,"HellmannExp",null,null,"DataElementValue"]
[null,"Amount",null,"DataElementName","DataElementValue"]
[null,"NominalDiscountRate",null,"DataElementName","DataElementValue"]
[null,null,null,null,null,"NonOperTimesElements"]
[null,null,null,null,null,"StartTime",null,null,"DataElementTimeValue"]
[null,"FinancingData",null,null,null,"EndTime",null,null,"DataElementTimeValue"]
[null,"AnnualInterest",null,"DataElementName","DataElementValue","StartTime",null,null,"DataElementIndex"]
[null,"LoanPeriodYears",null,"DataElementName","DataElementValue"]
[null,"LoanPeriodMonths",null,"DataElementName","DataElementValue","HeatPumpElements"]
[null,null,null,null,null,"ElectricalCapacity",null,null,"DataElementValue"]
[null,null,null,null,null,"MinElecCapacity",null,null,"DataElementValue"]
[null,"TaxationData",null,null,null,"MaxHeatCapacity",null,null,"DataElementValue"]
[null,"TaxRate",null,"DataElementName","DataElementValue","COP",null,null,"DataElementValue"]
[null,"LossCarriedForward",null,"DataElementName","DataElementValue","HeatedFrom",null,null,"DataElementValue"]
[null,null,null,null,null,"HeatedTo",null,null,"DataElementValue"]
[null,null,null,null,null,"CooledFrom",null,null,"DataElementValue"]
[null,"Output Types",null,null,null,"CooledTo",null,null,"DataElementValue"]
[null,"Text report","OutputReports","TextReportFileTypes",null,"HeatedFromExprStr",null,null,"DataElementValue"]
[null,"Graphic report","GraphicOutputReports","GraphicReportFileTypes",null,"HeatedToExprStr",null,null,"DataElementValue"]
[null,null,null,null,null,"CooledFromExprStr",null,null,"DataElementValue"]
[null,null,null,null,null,"CooledToExprStr",null,null,"DataElementValue"]
[null,"Output Reports",null,null,"ReportFileTypes","CutOffWhenCooled",null,null,"DataElementValue"]
[null,"EnergyConversionAnnual",null,null,"txt"]
[null,"EnergyConversionMonthly",null,null,"csv"]
[null,"EnergyConversionSummary",null,null,"pdf"]
[null,"Environment"]
[null,"ProductionPlan"]
[null,"CashFlowMonthly"]
[null,"CashFlowSummary",null,"Output Report Type"]
[null,"OperationIncome",null,"Report ID","ReportBaseID"]
[null,"FinancialKeyFigures",null,"COMPARE, name of alternative","AltName"]
[null,"IncomeStatement",null,"Report name","ReportFileName"]
[null,"IncomeStatementSummary",null,"Report extension","ReportFileType"]
[null,"BalanceSheet",null,"Report delimiter","ReportDelimiter"]
[null,"BalanceSheetSummary",null,"Report decimal separator","ReportDecimalSeparator"]
[null,"CatalogueTechnicalAssumptions",null,"Report Resolution","ReportResolution"]
[null,"CatalogueEconomicAssumptions",null,"Report start date","ReportStartDate","ReportFileType"]
[null,"OperationStrategyCalculation",null,"Report end date","ReportEndDate"]
[null,"ProjectReports"]
[null,"ToolsCopyEnergyConversion",null,null,"ReportResolution"]
[null,"CompareEnergyConversion",null,null,"Year"]
[null,"CompareCashFlow",null,null,"Month"]
[null,"CompareIncomeStatement",null,null,"Day"]
[null,"CompareFinancialKeyFigures",null,null,"Hour"]
[null,null,null,null,"Step"]
[]
[null,null,null,null,"Graphic ReportFileTypes"]
[null,null,null,null,"jpg"]
[null,"Graphic Output Reports"]
[null,"ProductionGraphic","ProductionGraphic"]
[null,"DurationCurveHeatDemand"]
[null,"DurationCurveProcessHeatDemand"]
[null,"DurationCurveElectricityDemand"]
[null,"DurationCurveCoolingDemand"]
[null,"CashFlowGraphic"]
[null,"GraphicalLayout"]
[null,"CompareKeyFiguresNetPresentValue"]
[null,"CompareKeyFiguresPayBackTime"]
[null,"CompareKeyFiguresIRR"]
[]
[]
[null,"ProductionGraphic"]
[null,"ReportStartDate"]
[null,"ReportEndDate"]

{"sheet":"Intro","index":5,"n_rows":67,"n_cols":2,"rows_kept":67,"cut":false,"hidden":true,"merged":[]}
["Example of calling energyPRO by xml"]
[]
[]
["energyPRO is called with the following parameters:"]
["c:\\Program Files\\Emd\\energyPRO 4\\energyPRO4.exe /XMLMod c:\\example.xml"]
[]
["/XMLMod is telling energyPRO that this is by xml"]
["The last parameter is the xml-file."]
[]
["This is an example of the content of an xml-file."]
["energyPRODataFile refers to the energyPRO file, which is to be altered."]
["The input data elements refer to the elements in the energyPRO, which are to be changed. In this case the demand \"Ab værk leverance\" and the payment \"Motor 1\" in the "]
["payment group \"Nox-afgifter\"."]
["Three report files will be saved."]
["<?xml version=\"1.0\" encoding=\"UTF-8\"?>"]
["<XMLtoEnergyPRO> "]
["<Head> "]
[null,"<energyPRODataFile>c:\\energyPRO data\\Dansk\\Danske eksempler\\Vestdansk 5MW-kraftvarmeværk på markedsvilkår i 2011.epp</energyPRODataFile> "]
[null,"<Version>1</Version> "]
[null,"<Date>01-06-2011</Date> "]
[]
["</Head> "]
["<InputDataElements>"]
[]
["   <InputDataElement> "]
["      <BaseID>500</BaseID> "]
["      <DataName>Ab værk leverance</DataName> "]
["      <DataElementName>Demand</DataElementName> "]
["      <DataElementValue>40000</DataElementValue> "]
["   </InputDataElement> "]
[]
["    <InputDataElement>      "]
["      <BaseID>800</BaseID>"]
["      <DataName>NOx-afgifter.Motor 1</DataName>"]
["      <DataElementName>amount</DataElementName>"]
["      <DataElementValue>0.03</DataElementValue> "]
["   </InputDataElement>"]
[]
["</InputDataElements> "]
[]
["<OutputDataElements> "]
[]
["   <OutputDataElement>      "]
["      <ReportBaseID>200</ReportBaseID>"]
["      <ReportDelimiter>;</ReportDelimiter>"]
["      <ReportFileName>c:\\Energy conversion, annual.txt</ReportFileName>"]
["      <ReportFileType>txt</ReportFileType>"]
["   </OutputDataElement>   "]
[]
["   <OutputDataElement>      "]
["      <ReportBaseID>100</ReportBaseID>"]
["      <ReportFileName>c:\\production, graphic1.jpg</ReportFileName>"]
["      <ReportFileType>jpg</ReportFileType>"]
["      <ReportStartDate>15-07-2011 00:00</ReportStartDate>"]
["      <ReportEndDate>23-07-2011 00:00</ReportEndDate>"]
["   </OutputDataElement>   "]
[]
["   <OutputDataElement>      "]
["      <ReportBaseID>10030</ReportBaseID>"]
["      <ReportDelimiter>;</ReportDelimiter>"]
["      <ReportFileName>c:\\OperationIncome.csv</ReportFileName>"]
["      <ReportFileType>csv</ReportFileType>"]
["   </OutputDataElement>   "]
[]
["</OutputDataElements>"]
[" "]
["</XMLtoEnergyPRO>"]

{"sheet":"BaseIDs","index":6,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":true,"merged":[]}
["InputData ","BaseID: ",100,"Project identification"]
["InputData ","BaseID: ",200,"External conditions"]
["InputData ","BaseID: ",205,"Time series"]
["InputData ","BaseID: ",210,"Time series functions","Not implemented"]
["InputData ","BaseID: ",215,"Indexes","Not implemented"]
["InputData ","BaseID: ",350,"Sites","Not implemented"]
["InputData ","BaseID: ",375,"Transmissions","Not implemented"]
["InputData ","BaseID: ",400,"Fuels"]
["InputData ","BaseID: ",500,"Demands"]
["InputData ","BaseID: ",600,"Energy conversion units"]
["InputData ","BaseID: ",650,"Storages"]
["InputData ","BaseID: ",690,"Electricity market"]
["InputData ","BaseID: ",700,"Operation strategy"]
["InputData ","BaseID: ",750,"Environment"]
["InputData ","BaseID: ",800,"Economy"]
["InputData ","BaseID: ",800,"Revenues"]
["InputData ","BaseID: ",800,"Operation expenditures"]
["InputData ","BaseID: ",840,"Investments"]
["InputData ","BaseID: ",850,"Financing"]
["InputData ","BaseID: ",860,"Taxation"]
["Reports ","BaseID: ",0,"Copy to clipboard"]
["Reports ","BaseID: ",100,"Production, graphic",null,null,null,"Graphical"]
["Reports ","BaseID: ",200,"Energy conversion, annual",null,null,null,"Text"]
["Reports ","BaseID: ",300,"Energy conversion, monthly"]
["Reports ","BaseID: ",350,"Energy conversion, summary"]
["Reports ","BaseID: ",400,"Duration curve for heat demand"]
["Reports ","BaseID: ",401,"Duration curve for process heat demand"]
["Reports ","BaseID: ",410,"Duration curve for electricity demand"]
["Reports ","BaseID: ",420,"Duration curve for cooling demand"]
["Reports ","BaseID: ",900,"Environment"]
["Reports ","BaseID: ",1000,"Production Plan"]
["Reports ","BaseID: ",10000,"Cash Flow, monthly"]
["Reports ","BaseID: ",10010,"Cash Flow, summary"]
["Reports ","BaseID: ",10020,"Cash flow, graphic"]
["Reports ","BaseID: ",10030,"Operation Income"]
["Reports ","BaseID: ",10040,"Financial Key Figures"]
["Reports ","BaseID: ",10060,"Income Statement"]
["Reports ","BaseID: ",10080,"Income Statement, summary"]
["Reports ","BaseID: ",10100,"Balance Sheet"]
["Reports ","BaseID: ",10110,"Balance Sheet, summary"]
["Reports ","BaseID: ",12000,"Catalogue of Technical Assumptions"]
["Reports ","BaseID: ",12100,"Catalogue of Economical Assumptions"]
["Reports ","BaseID: ",20000,"Operation Strategy Calculation"]
["Reports ","BaseID: ",20090,"Graphical Layout"]

{"sheet":"Parameters and examples","index":7,"n_rows":202,"n_cols":17,"rows_kept":202,"cut":false,"hidden":true,"merged":[]}
["ProjectIdentification",null,null,null,"Example"]
[null,"CalcPeriodLengthMinutes",null,null,"Modifying calculation step"]
[null,null,null,null,"   <InputDataElement> "]
[null,null,null,null,null,"<BaseID>100</BaseID> "]
[null,null,null,null,null,"<DataElementName>CalcPeriodLengthMinutes</DataElementName> "]
[null,null,null,null,null,"<DataElementValue>15</DataElementValue> "]
[null,null,null,null,"   </InputDataElement> "]
[]
[null,"OptimizationPeriodLength",null,null,"Modifying optimization period length"]
[null,null,null,null,"   <InputDataElement> "]
[null,null,null,null,null,"<BaseID>100</BaseID> "]
[null,null,null,null,null,"<DataElementName>OptimizationPeriodLength</DataElementName> "]
[null,null,null,null,null,"<DataElementValue>oplYear</DataElementValue> "]
[null,null,null,null,"   </InputDataElement> "]
[]
["External Conditions"]
[null,"CalcEnd",null,null,"Modifying calculation starttime"]
[null,null,null,null,"<InputDataElement>"]
[null,null,null,null,"<BaseID>200</BaseID>"]
[null,null,null,null,null,"<DataElementName>CalcStart</DataElementName>"]
[null,null,null,null,null,"<DataElementTimeValue>07-03-2000 00:00</DataElementTimeValue>"]
[null,null,null,null,"</InputDataElement>"]
[]
[null,"CalcStart",null,null,"Modifying calculation endtime"]
[null,null,null,null,"<InputDataElement>"]
[null,null,null,null,null,"<BaseID>200</BaseID>"]
[null,null,null,null,null,"<DataElementName>CalcEnd</DataElementName>"]
[null,null,null,null,null,"<DataElementTimeValue>14-03-2000 11:00</DataElementTimeValue>"]
[null,null,null,null,"</InputDataElement>"]
[]
["Time Series"]
[null,"TimeSeries",null,null,"Modifying time series by replacing with external file, here xml:",null,null,null,null,null,null,null,null,null,"xml data file:"]
[null,"File type:",null,null,"    <InputDataElement>      ",null,null,null,null,null,null,null,null,null,"<?xml version=\"1.0\" encoding=\"windows-1252\"?>"]
[null,"txt",null,null,null," <BaseID>205</BaseID>",null,null,null,null,null,null,null,null,"  <ePROTimeSeriesData>"]
[null,"csv",null,null,null,"<DataName>UdeTemp</DataName>"]
[null,"epw",null,null,null,"<DataElementName>weatherdata.TimeSeries</DataElementName>",null,null,null,null,null,null,null,null,"    <Head>"]
[null,"xml",null,null,null," <TimeSeriesFileName>c:\\temp\\xmltest\\Udetemp.xml</TimeSeriesFileName>",null,null,null,null,null,null,null,null,null,"<Date>28-10-2009  </Date>"]
[null,null,null,null,null,"<TimeSeriesFileType>xml</TimeSeriesFileType>",null,null,null,null,null,null,null,null,null,"<Filename>Atest-2 dage.xml </Filename>"]
[null,null,null,null,"   </InputDataElement>",null,null,null,null,null,null,null,null,null,"</Head>"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"<TimeSeriesElement>"]
[null,null,null,null,"epw:",null,null,null,null,null,null,null,null,null,null,"<DataName>UdeTemp</DataName> "]
[null,null,null,null,"    <InputDataElement>      ",null,null,null,null,null,null,null,null,null,null,"<DateFormat>dd-MM-yyyy hh:mm:ss</DateFormat> "]
[null,null,null,null,"      <BaseID>205</BaseID>",null,null,null,null,null,null,null,null,null,null,"<DateValueElements>"]
[null,null,null,null,"      <DataName>Elspot</DataName>",null,null,null,null,null,null,null,null,null,null,null,"<Data Time=\"01-01-2009 00:00:00\" Value=\"27.56\"></Data>"]
[null,null,null,null,"      <DataElementName>weatherdata.TimeSeries</DataElementName>",null,null,null,null,null,null,null,null,null,null,null,"<Data Time=\"01-01-2009 06:00:00:00\" Value=\"0.81\"></Data>"]
[null,null,null,null,"      <TimeSeriesFileName>c:\\ePxml\\ElspotVestdanmark2009.epw</TimeSeriesFileName>",null,null,null,null,null,null,null,null,null,null,null,"<Data Time=\"01-01-2009 21:00:00\" Value=\"0.56\"></Data>"]
[null,null,null,null,"      <TimeSeriesFileType>epw</TimeSeriesFileType>",null,null,null,null,null,null,null,null,null,null,null,"<Data Time=\"02-01-2009\" Value=\"34.65\"></Data>"]
[null,null,null,null,"   </InputDataElement>",null,null,null,null,null,null,null,null,null,null,null,"<Data Time=\"02-01-2009 06\" Value=\"38.81\"></Data>"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"<Data Time=\"02-01-08 21:00:00\" Value=\"34.65\"></Data>"]
[null,null,null,null,"csv:",null,null,null,null,null,null,null,null,null,null,null,"<Data Time=\"03-01-2009 00:00:00\" Value=\"31.19\"></Data>"]
[null,null,null,null,"    <InputDataElement>      ",null,null,null,null,null,null,null,null,null,null," </DateValueElements>"]
[null,null,null,null,"      <BaseID>205</BaseID>",null,null,null,null,null,null,null,null,null,"</TimeSeriesElement> "]
[null,null,null,null,"      <DataName>Elspot</DataName>",null,null,null,null,null,null,null,null,null,"  </ePROTimeSeriesData>"]
[null,null,null,null,"      <DataElementName>weatherdata.TimeSeries</DataElementName>"]
[null,null,null,null,"      <ReportDelimiter>;</ReportDelimiter>"]
[null,null,null,null,"      <TimeSeriesFileName>c:\\ePxml\\Elspot2011.csv</TimeSeriesFileName>"]
[null,null,null,null,"      <TimeSeriesFileType>csv</TimeSeriesFileType>"]
[null,null,null,null,"   </InputDataElement>"]
[]
["Demand"]
[null,"DaylyRatioFormular",null,null,"Modifying annual heat demand"]
[null,"Demand",null,null,"   <InputDataElement> "]
[null,"DemandFrom",null,null,null,"<BaseID>500</BaseID> "]
[null,"DemandTo",null,null,null,"<DataName>Heat Demand</DataName> "]
[null,"IncludedFrom",null,null,null,"<DataElementName>Demand</DataElementName> "]
[null,"IncludedTo",null,null,null,"<DataElementValue>99999</DataElementValue> "]
[null,"OutDoorTempSymbol",null,null,"   </InputDataElement> "]
[null,"ReferenceTemperature"]
[null,"SiteID",null,null,"Modifying weather dependency fraction:"]
[null,"WeatherDepFraction",null,null,"   <InputDataElement> "]
[null,"WeatherDepSeasonFrom",null,null,null,"<BaseID>500</BaseID> "]
[null,"WeatherDepSeasonTo",null,null,null,"<DataName>Heat Demand</DataName> "]
[null,null,null,null,null,"<DataElementName>WeatherDepFraction</DataElementName> "]
[null,null,null,null,null,"<DataElementValue>23</DataElementValue> "]
[null,null,null,null,"   </InputDataElement> "]
[]
[null,null,null,null,"Demand as time series:"]
[null,null,null,null,"   <InputDataElement>      "]
[null,null,null,null,null,"<BaseID>500</BaseID>"]
[null,null,null,null,null,"<DataName>HeatDemand</DataName>"]
[null,null,null,null,null,"<DataElementName>weatherdata.TimeSeries</DataElementName>"]
[null,null,null,null,null,"<TimeSeriesFileName>c:\\temp\\xmltest\\HeatDemand.epw</TimeSeriesFileName>"]
[null,null,null,null,null,"<TimeSeriesFileType>epw</TimeSeriesFileType>"]
[null,null,null,null,"   </InputDataElement>"]
[]
["Fuels"]
[null,"FuelContentPrimo",null,null,"content of fuel store primo calculation"]
[null,"FuelContentUltimo",null,null," <InputDataElement> "]
[null,"FuelStorage",null,null,null,"<BaseID>400</BaseID> "]
[null,"ThermalValue",null,null,null,"<DataName>Naturgas</DataName> "]
[null,"UnitName",null,null,null,"<DataElementName>FuelContentPrimo</DataElementName> "]
[null,null,null,null,null,"<DataElementValue>17</DataElementValue> "]
[null,null,null,null,"   </InputDataElement> "]
[null,null,null,null,"content of fuel store ultimo of calculation"]
[null,null,null,null,"   <InputDataElement> "]
[null,null,null,null,null,"<BaseID>400</BaseID> "]
[null,null,null,null,null,"<DataName>Naturgas</DataName> "]
[null,null,null,null,null,"<DataElementName>FuelContentUltimo</DataElementName> "]
[null,null,null,null,null,"<DataElementValue>21</DataElementValue> "]
[null,null,null,null,"   </InputDataElement> "]
[]
["Energy conversion units"]
[null,"NonOperTimes",null,null,"Start of first non operation period"]
[null,"OperationalFrom",null,null,"<InputDataElement>"]
[null,"OperationalTo",null,null,null,"<BaseID>600</BaseID>"]
[null,"PowerCurve",null,null,null,"<DataName>Motor1</DataName>"]
[null,"ShutDownPeriod",null,null,null,"<DataElementName>NonOperTimes.StartTime</DataElementName>"]
[null,"SolarUnit",null,null,null,"<DataElementIndex>1</DataElementIndex>"]
[null,"StartUpPeriod",null,null,null,"<DataElementTimeValue>01-01-2012 12:00</DataElementTimeValue>"]
[null,"WindFarm",null,null,"</InputDataElement>"]
[]
[null,"PowerCurve:",null,null,"End of first non operation period"]
[null,"CoolProd",null,null,"<InputDataElement>"]
[null,"ElCon",null,null,null,"<BaseID>600</BaseID>"]
[null,"ElProd",null,null,null,"<DataName>Motor1</DataName>"]
[null,"Fuel",null,null,null,"<DataElementName>NonOperTimes.EndTime</DataElementName>"]
[null,"HeatCon",null,null,null,"<DataElementIndex>1</DataElementIndex>"]
[null,"HeatProd",null,null,null,"<DataElementTimeValue>02-01-2012 17:00</DataElementTimeValue>"]
[null,"ProcHeatCon",null,null,"</InputDataElement>"]
[null,"ProcHeatProd"]
[null,null,null,null,"Power curve value"]
[null,"SolarUnit:",null,null,"<InputDataElement>"]
[null,"IncidenceAngleMod50",null,null,null,"<BaseID>600</BaseID>"]
[null,"IncidenceAngleModCoef",null,null,null,"<DataName>Motor1</DataName>"]
[null,"IncidenceAngleModSavedAsCoeff",null,null,null,"<DataElementName>PowerCurve.Fuel</DataElementName>"]
[null,"Inclination",null,null,null,"<DataElementValue>3669</DataElementValue>"]
[null,"InstalledElecCapacity",null,null,"</InputDataElement>"]
[null,"K0"]
[null,"K1",null,null,"Solar collector area"]
[null,"Lattitude",null,null,"<InputDataElement>"]
[null,"N0",null,null,null,"<BaseID>600</BaseID>"]
[null,"NOCT",null,null,null,"<DataName>Solfanger</DataName>"]
[null,"Orientation",null,null,null,"<DataElementName>SolarUnit.TotalArea</DataElementName>"]
[null,"PMax",null,null,null,"<DataElementValue>9876</DataElementValue>"]
[null,"PowerLosses",null,null,"</InputDataElement>"]
[null,"ReflectionFactor"]
[null,"TempCoeffPower"]
[null,"TemperatureAvg"]
[null,"TotalArea"]
[]
[null,"WindFarm"]
[null,"AnnualProduction"]
[null,"Conversiontable"]
[null,"HellmannExp"]
[null,"HubHeight"]
[null,"MeasureHeight"]
[null,"ScaleType"]
[null,"ScaleValue"]
[null,"WindFarmCalcType"]
[null,"WindTSID"]
[]
[]
["Stores"]
[null,"PrimoStorage",null,null,"Storage content, start"]
[null,"StorageUtilization",null,null,"   <InputDataElement> "]
[null,"UltimoStorage",null,null,null,"<BaseID>650</BaseID> "]
[null,null,null,null,null,"<DataName>Varmelager</DataName> "]
[null,null,null,null,null,"<DataElementName>PrimoStorage</DataElementName> "]
[null,null,null,null,null,"<DataElementValue>11</DataElementValue> "]
[null,null,null,null,"   </InputDataElement> "]
[]
[null,null,null,null,"Storage content, end"]
[null,null,null,null,null,"<BaseID>650</BaseID> "]
[null,null,null,null,null,"<DataName>Varmelager</DataName> "]
[null,null,null,null,null,"<DataElementName>UltimoStorage</DataElementName> "]
[null,null,null,null,null,"<DataElementValue>12</DataElementValue> "]
[null,null,null,null,"   </InputDataElement>"]
[]
["Payments"]
[null,"Amount",null,null,"Amount (price per unit):"]
[null,null,null,null,"    <InputDataElement>      "]
[null,null,null,null,null,"      <BaseID>800</BaseID>"]
[null,null,null,null,null,"      <DataName>NOx-afgifter.Motor 1</DataName>"]
[null,null,null,null,null,"      <DataElementName>amount</DataElementName>"]
[null,null,null,null,null,"      <DataElementValue>0.03</DataElementValue> "]
[null,null,null,null,"   </InputDataElement>"]
[]
["Reports"]
[null,null,null,null,"Energy conversion, annual:"]
[null,null,null,null,"   <OutputDataElement>      "]
[null,null,null,null,"      <ReportBaseID>200</ReportBaseID>"]
[null,null,null,null,"      <ReportDelimiter>;</ReportDelimiter>"]
[null,null,null,null,"      <ReportFileName>c:\\Energy conversion, annual.txt</ReportFileName>"]
[null,null,null,null,"      <ReportFileType>txt</ReportFileType>"]
[null,null,null,null,"   </OutputDataElement>   "]
[]
[null,null,null,null,"Production, graphic:"]
[null,null,null,null,"   <OutputDataElement>      "]
[null,null,null,null,"      <ReportBaseID>100</ReportBaseID>"]
[null,null,null,null,"      <ReportFileName>c:\\production, graphic1.jpg</ReportFileName>"]
[null,null,null,null,"      <ReportFileType>jpg</ReportFileType>"]
[null,null,null,null,"      <ReportStartDate>15-07-2011 00:00</ReportStartDate>"]
[null,null,null,null,"      <ReportEndDate>23-07-2011 00:00</ReportEndDate>"]
[null,null,null,null,"   </OutputDataElement>   "]
[]
[null,null,null,null,"Operation Income:"]
[null,null,null,null,"   <OutputDataElement>      "]
[null,null,null,null,"      <ReportBaseID>10030</ReportBaseID>"]
[null,null,null,null,"      <ReportDelimiter>;</ReportDelimiter>"]
[null,null,null,null,"      <ReportFileName>c:\\OperationIncome.csv</ReportFileName>"]
[null,null,null,null,"      <ReportFileType>csv</ReportFileType>"]
[null,null,null,null,"   </OutputDataElement>   "]